{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":10,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","GM R290"]
[]
[]
[]
[]
["","","","","","BGM0870Y1ACA","MGM1280Y1ACA","MGM2210Y1ACA","BGM0870Y1WAA","MGM1280Y1WAA"]
["Koelvermogen","Lage temperatuur","R-290","Nom","kW","0.871","","","0.871"]
["","Matige temperatuur","R-290","Nom","kW","","1.281","2.206","","1.281"]
["Behuizing","Kleur","","Condensorunit","","Grijs","Grijs","Grijs","Grijs","Grijs"]
["Afmetingen","Unit","","Hoogte","mm","735","735","830","735","735"]
["","","","Breedte","mm","400","400","620","400","400"]
["","","","Diepte","mm","790","790","790","790","790"]
["Gewicht","Unit","","","kg","64","56","80","64","56"]
["Compressor","Hoeveelheid","","","","1","1","1","1","1"]
["","Type","","","","Dampcompressie","Dampcompressie","Dampcompressie","Dampcompressie","Dampcompressie"]
["","Model","","","","NT2180UV","NEU6217U","NTX6225UV","NT2210U/CSR","NT6220U/CSR"]
["","Aanloopmethode_","","","","Rechtstreeks","Rechtstreeks","Rechtstreeks","Rechtstreeks","Rechtstreeks"]
["Condensor","Luchtdebiet","","","m³/u","600","600","1,200","600","600"]
["Ontdooiing","","","","","Heet gas","Heet gas","Heet gas","Heet gas","Heet gas"]
["Verdamper","Luchtuitblaasbereik","","","m","4","4","4","4","4"]
["Werkingsbereik","Temperatuur koelkamer","","Min.","°C","-25","-5","-5","-25","-5"]
["","","","Max.","°C","-15","10","10","-15","10"]
["Werkbereik","Omgevingstemperatuur","","Min.","°C","20","20","20","20","20"]
["Werkingsbereik","Omgevingstemperatuur","","Max.","°C","45","45","45","45","45"]
["Koelmiddel","Type","","","","R-290","R-290","R-290","R-290","R-290"]
["","GWP","","","","3","3","3","3","3"]
["Spanningsvoeding","Spanning","","","V","220-230","220-230","220-230","220-230","220-230"]
["Voeding","Fase","","","","1~","1~","1~","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","60","60","60","50","50"]