{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":58,"n_cols":7,"rows_kept":58,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","JEHCCU-CM3"]
[]
[]
[]
[]
["","","","","","JEHCCU0140CM3","JEHCCU0170CM3"]
["Koelvermogen","Gemiddelde temperatuur","R-407F","Nom","kW","2.08"]
["Koelcapaciteit","Middelhoge temperatuur","R-449A","Nom.","kW","2.15","2.57"]
["Koelvermogen","Gemiddelde temperatuur","R-407A","Nom","kW","1.92"]
["Koelcapaciteit","Middelhoge temperatuur","R-448A","Nom.","kW","2.15","2.57"]
["Opgenomen vermogen","Matige temperatuur","R-407F","Nom","kW","1.12"]
["","","R-407A","Nom","kW","1.16"]
["","Middelhoge temperatuur","R-448A","Nom.","kW","1.07","1.46"]
["","","R-449A","Nom.","kW","1.07","1.46"]
["Prestatiecoëfficiënt (COP)","Middelhoge temperatuur","","R-448A","","2","1.76"]
["","","","R-449A","","2","1.76"]
["","","","R-407F","","1.85"]
["","","","R-407A","","1.66"]
["Parameters bij vollast en omgevingstemp. 32°C (punt A)","R-407A","Te -10°C","Nom. koelvermogen (PA)","kW","1.92"]
["","","","Nom. opgenomen vermogen (DA)","kW","1.16"]
["","","","Nom. COP (COPA)","","1.66"]
["","R-407F","Te -10°C","Nom. koelvermogen (PA)","kW","2.08"]
["","","","Nom. opgenomen vermogen (DA)","kW","1.12"]
["","","","Nom. COP (COPA)","","1.85"]
["","R-448A","Te -10°C","Nom. koelvermogen (PA)","kW","2.15","2.57"]
["","","","Nom. opgenomen vermogen (DA)","kW","1.07","1.46"]
["","","","Nom. COP (COPA)","","2","1.76"]
["","R-449A","Te -10°C","Nom. koelvermogen (PA)","kW","2.15","2.57"]
["","","","Nom. opgenomen vermogen (DA)","kW","1.07","1.46"]
["","","","Nom. COP (COPA)","","2","1.76"]
["Parameters bij vollast en omgevingstemp. 25°C","R-407A","Te -10°C","Vermelde COP (COP2)","","1.78"]
["","R-407F","Te -10°C","Vermelde COP (COP2)","","2.11"]
["","R-448A","Te -10°C","Opgenomen vermogen (D2)","kW","1.02","1.4"]
["","","","Vermelde COP (COP2)","","2.31","2.01"]
["","R-449A","Te -10°C","Opgenomen vermogen (D2)","kW","1.02","1.4"]
["","","","Vermelde COP (COP2)","","2.31","2.01"]
["Parameters bij vollast en omgevingstemp. 43°C","R-407A","Te -10°C","Vermelde COP (COP3)","","1.48"]
["","R-407F","Te -10°C","Vermelde COP (COP3)","","1.49"]
["","R-448A","Te -10°C","Vermelde COP (COP3)","","1.53","1.43"]
["","R-449A","Te -10°C","Vermelde COP (COP3)","","1.53","1.43"]
["Ventilator","Type","","","","Axiaal","Axiaal"]
["Afmetingen","Unit","","Hoogte","mm","662","662"]
["","","","Breedte","mm","1101","1101"]
["","","","Diepte","mm","444","444"]
["Gewicht","Unit","","","kg","67","68"]
["Behuizing","Kleur","","","","Lichtgrijs","Lichtgrijs"]
["Koelmiddel","Type 2","","","","R-407A"]
["","Type 3","","","","R-407F"]
["","Type 5","","","","R-448A","R-448A"]
["","GWP type 5","","","","1387","1387"]
["","GWP type 2","","","","2107"]
["","GWP type 3","","","","1825"]
["Voeding","Fase","","","","3~","3~"]
["Spanningsvoeding","Frequentie","","","Hz","50","50"]
["","Spanning","","","V","400","400"]
["Opmerkingen","","","","","(1) - SRG 20°C, Ta=32°C, Te=-35°C","(1) - SRG 20°C, Ta=32°C, Te=-35°C"]
["","","","","","(2) - Geluidsdruk wordt gemeten op 10 m in anti-echo-kamer.","(2) - Geluidsdruk wordt gemeten op 10 m in anti-echo-kamer."]
["","","","","","(3) - Werkt op gefluoreerde broeikasgassen","(3) - Werkt op gefluoreerde broeikasgassen"]