{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","LRMEQ-BY1"]
[]
[]
[]
[]
["","","","","","LRMEQ3BY1","LRMEQ4BY1"]
["Standaard-accessoires","Montagehandleiding","","","","Montagehandleiding","Montagehandleiding"]
["","Algemene voorzorgsmaatregelen","","","","Algemene voorzorgsmaatregelen","Algemene voorzorgsmaatregelen"]
["","Koelmiddellabel voor wetgeving inzake F-gas","","","","Koelmiddellabel voor wetgeving inzake F-gas","Koelmiddellabel voor wetgeving inzake F-gas"]
["","Hulpleidingenset","","","","Hulpleidingenset","Hulpleidingenset"]
["","Stickervel met F-gaslabel","","","","Stickervel met F-gaslabel","Stickervel met F-gaslabel"]
["","Productfiche Ecodesign","","","","Productfiche Ecodesign","Productfiche Ecodesign"]
["Koelcapaciteit","Middelhoge temperatuur","","kW","kW","5.90 (1)","8.40 (1)"]
["Gewicht","Unit","","","kg","126","126"]
["Koelmiddel","Charge","","","TCO2Eq","9.39","9.39"]
["","GWP","","","","2,087.5","2,087.5"]
["","Vulling","","","kg","4.50","4.50"]
["","Type","","","","R-410A","R-410A"]
["Ventilatormotor","Uitgang","","","W","70","70"]
["","Aandrijving","","","","Directe aandrijving","Directe aandrijving"]
["Warmtewisselaar","Type","","","","Kruiselings geribd blok","Kruiselings geribd blok"]
["Opgenomen vermogen","Middelhoge temperatuur","","Nom.","kW","2.53 (1)","3.65 (1)"]
["COP","Medium temperature","","Nom.","","2.33 (1)","2.30 (1)"]
["Afmetingen","Unit","","Breedte","mm","900","900"]
["","","","Diepte","mm","320","320"]
["","","","Hoogte","mm","1,345","1,345"]
["Behuizing","Kleur","","","","Daikin wit","Daikin wit"]
["Ventilator","Type","","","","Schroef","Schroef"]
["","Luchtdebiet","Koelen","Nom.","m³/min","106","106"]
["","Aantal","","","","2","2"]
["Power supply","Fase","","","","3N~","3N~"]
["","Frequentie","","","Hz","50","50"]
["","Spanning","","","V","380-415","380-415"]
["Opmerkingen","","","","","(1) - Koelen: verdamping -10°C; buitentemp. 32°C; aanzuiging SH10°C","(1) - Koelen: verdamping -10°C; buitentemp. 32°C; aanzuiging SH10°C"]
["","","","","","(2) - Geluidsdruk: gemeten op 1 meter afstand van de voorkant van de unit, op een hoogte van 1,5 m.","(2) - Geluidsdruk: gemeten op 1 meter afstand van de voorkant van de unit, op een hoogte van 1,5 m."]
["","","","","","(3) - Bevat gefluoreerde broeikasgassen","(3) - Bevat gefluoreerde broeikasgassen"]