{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":6,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC30YV"]
[]
[]
[]
[]
["","","","","","MC30YVM"]
["Type","","","","","Luchtreiniger"]
["Toepassing","","","","","Vloermodel"]
["Omkasting","Colour","","","","Wit"]
["Afmetingen","Unit","","Hoogte","mm","450"]
["","","","Breedte","mm","270"]
["","","","Diepte","mm","270"]
["Gewicht","Unit","","","kg","5.8"]
["Geschikt voor vloeroppervlakte","m²","","","","23 (1), 46 (2)"]
["CADR","m³/u","","","","180"]
["Werking luchtreiniging","Opgenomen vermogen","","Turbo","kW","0.025"]
["","","","M","kW","0.015"]
["","","","Fluisterstil","kW","0.008"]
["Geluidsdrukniveau","Werking luchtreiniging","","Turbo","dBA","37"]
["","","","Middelhoog","dBA","27"]
["","","","Fluisterstil","dBA","19"]
["Ventilator","Luchtdebiet","Werking luchtreiniging","Turbo","m³/u","180"]
["","","","Middelhoog","m³/u","120"]
["","","","Fluisterstil","m³/u","60"]
["Stofvangmethode","","","","","Elektrostatisch HEPA-filter"]
["Deodorizing method","","","","","Flash streamer + ontgeurende katalysator"]
["Standaard-accessoires","Elektrostatisch HEPA-filter","","","","1"]
["","Geurfilter","","","","1"]
["","Bedieningshandleiding","","","","1"]
["Voedingskabel","m","","","","1.8"]
["Power supply","Fase","","","","1~"]
["","Frequentie","","","Hz","50/60"]
["","Spanning","","","V","220-240/220-230"]
["Bedrijfsstroom","Werking luchtreiniging","","Turbo","A","0.13"]
["","","","Middelhoog","A","0.09"]
["","","","Fluisterstil","A","0.08"]
["Opmerkingen","","","","","(1) - De betreffende vloeroppervlakte is voldoende voor het gebruiken van de unit met maximaal toerental van de ventilator (HH). De betreffende vloeroppervlakte verwijst naar de ruimte waarin een bepaald gedeelte stofdeeltjes verwijderd kan worden op 30 minuten. (JEM 1467)"]
["","","","","","(2) - De toepasselijke kameroppervlakte verwijst naar de werking van de unit met maximaal ventilatortoerental (HH). De toepasselijke kameroppervlakte werd berekent overeenkomstig de norm NRCC-54013 door middel van sigarettenrook CADR die werd getest overeenkomstig JEM1467."]
["","","","","","(3) - Omgezet naar CADR-normen van testwaarden overeenkomstig JEM1467."]
["","","","","","(4) - De geluidsniveaus zijn het gemiddelde van de waarden gemeten op 1 m afstand van de voorkant, linker- en rechterkant en achterkant van de unit. (Deze zijn gelijk aan de waarde in een echoloze ruimte)"]
["","","","","","(5) - Een elektrostatisch HEPA-filter is opgenomen in de unit."]
["","","","","","(6) - Andere functie: Automatische herstartfunctie."]