{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MC80Z"]
[]
[]
[]
[]
["","","","","","MC80ZVM"]
["Type","","","","","Luchtreiniger"]
["Toepassing","","","","","Vloermodel"]
["Behuizing","Kleur","","","","Front: White, Top/Side: Dark Grey"]
["Afmetingen","Unit","","Hoogte","mm","630"]
["","","","Breedte","mm","315"]
["","","","Diepte","mm","315"]
["Gewicht","Unit","","","kg","9.8"]
["Geschikt voor vloeroppervlakte","m²","","","","62, 124"]
["CADR","m³/u","","","","480"]
["Werking luchtreiniging","Opgenomen vermogen","","Turbo","kW","0.080"]
["","","","M","kW","0.016"]
["","","","L","kW","0.011"]
["","","","Fluisterstil","kW","0.009"]
["Geluidsdrukniveau","Werking luchtreiniging","","Turbo","dBA","55"]
["","","","Middelhoog","dBA","34"]
["","","","Laag","dBA","25"]
["","","","Fluisterstil","dBA","19"]
["Ventilator","Luchtdebiet","Werking luchtreiniging","Turbo","m³/u","480"]
["","","","Middelhoog","m³/u","210"]
["","","","Laag","m³/u","132"]
["","","","Fluisterstil","m³/u","84"]
["Stofvangmethode","","","","","Elektrostatisch HEPA-filter"]
["Ontgeuringsmethode","","","","","Dubbele streamer + geurkatalysator"]
["Standaard-accessoires","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["Voedingskabel","m","","","","2"]
["Voeding","Fase","","","","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50/60"]
["","Spanning","","","V","220-240/220-230"]
["Opmerkingen","","","","","(1) - De gedekte oppervlakte is geschikt voor het gebruiken van de unit met maximaal ventilatortoerental (HH). De gedekte oppervlakte geeft de ruimte aan waarin een bepaalde hoeveelheid stofdeeltjes in 30 minuten verwijderd kan worden."]
["","","","","","(2) - Omgezet naar NRCC-normen van testwaarden overeenkomstig JEM1467."]