{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":6,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK555A"]
[]
[]
[]
[]
["","","","","","MCK555AVM-W"]
["Type","","","","","Luchtbevochtiger en -reiniger"]
["Toepassing","","","","","Vloermodel"]
["Behuizing","Kleur","","","","Wit (N9. 0)"]
["Afmetingen","Unit","","Hoogte","mm","700"]
["","","","Breedte","mm","270"]
["","","","Diepte","mm","270"]
["Gewicht","Unit","","","kg","9.5"]
["Geschikt voor vloeroppervlakte","m²","","","","41 (1), 82 (2)"]
["CADR-=-m³/u","m³/u","","","","320"]
["Werking luchtreiniging","Opgenomen vermogen","","Turbo","kW","0.056"]
["","","","M","kW","0.017"]
["","","","L","kW","0.010"]
["","","","Fluisterstil","kW","0.007"]
["Bevochtiging","Opgenomen vermogen","","Turbo","kW","0.058"]
["","","","M","kW","0.019"]
["","","","L","kW","0.014"]
["","","","Fluisterstil","kW","0.009"]
["","Inhoud waterreservoir","","","l","2.7"]
["Geluidsdrukniveau","Werking luchtreiniging","","Turbo","dBA","53"]
["","","","Middelhoog","dBA","39"]
["","","","Laag","dBA","29"]
["","","","Fluisterstil","dBA","20"]
["","Bevochtiging","","Turbo","dBA","53"]
["","","","Middelhoog","dBA","39"]
["","","","Laag","dBA","33"]
["","","","Fluisterstil","dBA","20"]
["Ventilator","Luchtdebiet","Werking luchtreiniging","Turbo","m³/u","330"]
["","","","Middelhoog","m³/u","192"]
["","","","Laag","m³/u","120"]
["","","","Fluisterstil","m³/u","54"]
["","","Bevochtiging","Turbo","m³/u","330"]
["","","","Middelhoog","m³/u","192"]
["","","","Laag","m³/u","144"]
["","","","Fluisterstil","m³/u","54"]
["Stofvangmethode","","","","","Elektrostatisch HEPA-filter"]
["Ontgeuringsmethode","","","","","Flash streamer + ontgeurende katalysator"]
["Standaard-accessoires","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Remote controller","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","2"]
["","Remote control holder","","","","1"]
["Voedingskabel","m","","","","1.8"]
["Voeding","Fase","","","","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50/60"]
["","Spanning","","","V","220-240/220-230"]
["Opmerkingen","","","","","(1) - De gedekte oppervlakte is geschikt voor het gebruiken van de unit met maximaal ventilatortoerental (HH). De gedekte oppervlakte geeft de ruimte aan waarin een bepaalde hoeveelheid stofdeeltjes in 30 minuten verwijderd kan worden."]
["","","","","","(2) - Omgezet naar NRCC-normen van testwaarden overeenkomstig JEM1467."]
["","","","","","(3) - Omgezet naar CADR-normen van testwaarden overeenkomstig JEM1467."]
["","","","","","(4) - De bevochtigingsgraad wijzigt in verhouding tot de temperatuur en luchtvochtigheid die binnen en buiten heerst. Meetomstandigheden: temperatuur 20°C, vochtigheid 30%."]
["","","","","","(5) - De geluidsniveaus zijn het gemiddelde van de waarden gemeten op 1 m afstand van de voorkant, linker- en rechterkant en achterkant van de unit. (Deze zijn gelijk aan de waarde in een echoloze ruimte)"]
["","","","","","(6) - Een elektrostatisch HEPA-filter en bevochtigingsfilters zijn opgenomen in de unit."]
["","","","","","(7) - Vereisten overeenkomstig JEM1467."]