{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":8,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXA-A9"]
[]
[]
[]
[]
["","","","","","RXA20A5V1B9 (Archived)","RXA25A5V1B9 (Archived)","RXA35A5V1B9 (Archived)"]
["Afmetingen","Unit","","Hoogte","mm","550","550","550"]
["","","","Breedte","mm","840","840","840"]
["","","","Diepte","mm","350","350","350"]
["Gewicht","Unit","","","kg","32","32","32"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkbereik","Koelen","Omgeving","Min.","°CDB","-10","-10","-10"]
["","","","Max.","°CDB","46","46","46"]
["","Verwarmen","Omgeving","Min.","°CWB","-15","-15","-15"]
["","","","Max.","°CWB","18","18","18"]
["Geluidsdrukniveau","Koelen","","Nom.","dBA","46.0","46.0","49.0"]
["","Verwarmen","","Nom.","dBA","47.0","47.0","49.0"]
["Koelmiddel","Type","","","","R-32","R-32","R-32"]
["","Vulling","","","kg","0.76","0.76","0.76"]
["Koudemiddel","Vulling","","","tCO2Eq","0.52","0.52","0.52"]
["Koelmiddel","GWP","","","","675.0","675.0","675.0"]
["Leidingaansluitingen","Leidinglengte","Max.","OU - IU","m","20","20","20"]
["","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)"]
["","Niveauverschil:","IU - OU","Max.","m","15.0","15.0","15.0"]
["Standaard-accessoires","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","Drain plug","","","","1","1","1"]
["Voeding","Fase","","","","1~","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-240"]