{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":63,"n_cols":9,"rows_kept":63,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXG-L"]
[]
[]
[]
[]
["","","","","","RXG20L2V1B","RXG25L2V1B","RXG35L2V1B","RXG50L2V1B"]
["Geluidsdrukniveau","Verwarmen","","Hoog","dBA","","47","48"]
["","Koelen","","Hoog","dBA","","46","48"]
["Standaard-accessoires","Koppeling (afvoer)","","","","","1","1"]
["","Montagehandleiding","","","","","1","1"]
["Koelmiddel","Charge","","","TCO2Eq","","2.2","2.2"]
["","GWP","","","","","2,087.5","2,087.5"]
["","Vulling","","","kg","","1.05","1.05"]
["","Type","","","","","R-410A","R-410A"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","tpm","","780","780"]
["","","Verwarmen","Superlaag","tpm","","740","740"]
["Leidingaansluitingen","Niveauverschil:","IU - OU","Max.","m","","15","15"]
["","Bijkomende koelmiddelvulling","","","kg/m","","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)"]
["Compressor","Type","","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Afmetingen","Unit","","Breedte","mm","","765","765"]
["","","","Diepte","mm","","285","285"]
["","","","Hoogte","mm","","550","550"]
["Gewicht","Unit","","","kg","","35","35"]
["Ventilator","Luchtdebiet","Verwarmen","Superlaag","cfm","","932","932"]
["","","Koelen","Superlaag","cfm","","1,094","1,094"]
["Power supply","Phase","","","","","1~","1~"]
["","Frequentie","","","Hz","","50","50"]
["","Spanning","","","V","","220-240","220-240"]
["Opmerkingen","","","","","(1) - 220V","(1) - SL: de geluidsarme instelling van de ventilator van de luchtcirculatie","(1) - SL: de geluidsarme instelling van de ventilator van de luchtcirculatie","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 220V","(2) - 220V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 230V","(3) - 230V","(3) - 240V"]
["","","","","","(4) - Bedrijfsbereik in combinatie met Nexura, FVXG-K, koeling: min. 10°C DB - max. 46°C DB; verwarming: min. -15°C NB - max. 18°C NB","(4) - 240V","(4) - 240V","(4) - Bedrijfsbereik in combinatie met Nexura, FVXG-K, koeling: min. 10°C DB - max. 46°C DB; verwarming: min. -15°C NB - max. 18°C NB"]
["","","","","","","(5) - Bedrijfsbereik in combinatie met Nexura, FVXG-K, koeling: min. 10°C DB - max. 46°C DB; verwarming: min. -15°C NB - max. 18°C NB","(5) - Bedrijfsbereik in combinatie met Nexura, FVXG-K, koeling: min. 10°C DB - max. 46°C DB; verwarming: min. -15°C NB - max. 18°C NB"]
["","","","","","","(6) - Bevat gefluoreerde broeikasgassen","(6) - Bevat gefluoreerde broeikasgassen"]
["Ventilator","Luchtdebiet","Koelen","Superlaag","m³/min","31.0","","","42.6"]
["","","Verwarmen","Superlaag","m³/min","26.4","","","38.3"]
["","","","Superlaag","cfm","1094","","","1504"]
["","","Verwarmen","Superlaag","cfm","932","","","1352"]
["Afmetingen","Unit","","Hoogte","mm","550","","","735"]
["","","","Breedte","mm","765","","","825"]
["","","","Diepte","mm","285","","","300"]
["Gewicht","Unit","","","kg","35","","","48"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","tpm","780","","","670"]
["","","Verwarmen","Superlaag","tpm","740","","","670"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","","","Hermetisch gesloten swingcompressor"]
["Werkbereik","Koelen","Omgeving","Min.","°CDB","-10 (5)","","","-10 (5)"]
["","","","Max.","°CDB","46","","","46"]
["","Verwarmen","Omgeving","Min.","°CWB","-15","","","-15"]
["","","","Max.","°CWB","18","","","18"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","46","","","48"]
["","Verwarmen","","Hoog","dBA","47","","","48"]
["Koelmiddel","Type","","","","R-410A","","","R-410A"]
["","Vulling","","","kg","1.05","","","1.6"]
["Koudemiddel","Vulling","","","tCO2Eq","2.2","","","3.3"]
["Koelmiddel","GWP","","","","2087.5","","","2087.5"]
["Leidingaansluitingen","Leidinglengte","Max.","OU - IU","m","20","","","30"]
["","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 10 m)","","","0,02 (voor leidinglengte van meer dan 10 m)"]
["","Niveauverschil:","IU - OU","Max.","m","15","","","20"]
["Standaard-accessoires","Installation manual","","","","1","","","1"]
["","Joint (drain)","","","","1","","","1"]
["Voeding","Fase","","","","1~","","","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50","","","50"]
["","Spanning","","","V","220-240","","","220-240"]