{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":16,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXJ-M"]
[]
[]
[]
[]
["","","","","","RXJ50MV1B","RXJ50M2V1B","RXJ20M2V1B (Archived)","RXJ20M3V1B (Archived)","RXJ20M5V1B (Archived)","RXJ25M2V1B (Archived)","RXJ25M3V1B (Archived)","RXJ25M5V1B (Archived)","RXJ35M2V1B (Archived)","RXJ35M3V1B (Archived)","RXJ35M5V1B (Archived)"]
["Ventilator","Luchtdebiet","Koelen","Superlaag","m³/min","38.5","","29.3","","","29.3","","","29.3"]
["","","Verwarmen","Superlaag","m³/min","34.3","","25.6","","","25.6","","","25.6"]
["","","","Superlaag","cfm","1359","","1035","","","1035","","","1035"]
["","","Verwarmen","Superlaag","cfm","1211","","904","","","904","","","904"]
["Afmetingen","Unit","","Hoogte","mm","735","735","550","550","550","550","550","550","550","550","550"]
["","","","Breedte","mm","825","825","765","765","765","765","765","765","765","765","765"]
["","","","Diepte","mm","300","300","285","285","285","285","285","285","285","285","285"]
["Gewicht","Unit","","","kg","44","44","34","32","32","34","32","32","34","32","32"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","tpm_","620","","760","","","760","","","760"]
["","","Verwarmen","Superlaag","tpm_","620","","740","","","740","","","740"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkbereik","Koelen","Omgeving","Min.","°CDB","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10","-10"]
["","","","Max.","°CDB","46","46","46","46","46","46","46","46","46","46","46"]
["","Verwarmen","Omgeving","Min.","°CWB","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15"]
["","","","Max.","°CWB","18","20","18","18","18","18","18","18","18","18","18"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","48","48","46","","","46","","","48"]
["","","","Nom.","dBA","","","","46","46","","46","46","","49","49"]
["","","","Laag","dBA","","45"]
["","Verwarmen","","Hoog","dBA","48","48","47","","","47","","","48"]
["","","","Nom.","dBA","","","","47","47","","47","47","","49","49"]
["","","","Laag","dBA","","45"]
["Koelmiddel","Type","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Vulling","","","kg","1.30","1.3","0.72","0.76","0.76","0.72","0.76","0.76","0.72","0.76","0.76"]
["Koudemiddel","Vulling","","","tCO2Eq","0.9","0.88","0.5","0.52","0.52","0.5","0.52","0.52","0.5","0.52","0.52"]
["Koelmiddel","GWP","","","","675","675","675","675.0","675.0","675","675.0","675.0","675","675.0","675.0"]
["Leidingaansluitingen","Leidinglengte","Max.","OU - IU","m","30","30","20","20","20","20","20","20","20","20","20"]
["","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 10 m)","","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)"]
["","Niveauverschil:","IU - OU","Max.","m","20","","15","15.0","15.0","15","15.0","15.0","15","15.0","15.0"]
["Standaard-accessoires","Installation manual","","","","1","","1","1","","1","1","","1","1"]
["","Drain plug","","","","1","","1","1","","1","1","","1","1"]
["Voeding","Fase","","","","1~","","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50","","50","50","50","50","50","50","50","50","50"]
["","Spanning","","","V","220-240","","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Opmerkingen","","","","","(1) - 220V","","(1) - 220V","","","(1) - 220V","","","(1) - 220V"]
["","","","","","(2) - 230V","","(2) - 230V","","","(2) - 230V","","","(2) - 230V"]
["","","","","","(3) - 240V","","(3) - 240V","","","(3) - 240V","","","(3) - 240V"]
["Standaard-accessoires","Refrigerant charge label","","","","","","","1","","","1","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","","","","1","","","1","","","1"]
["","General safety precautions","","","","","","","1","","","1","","","1"]