{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":8,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-A9"]
[]
[]
[]
[]
["","","","","","RXM25A5V1B9","RXM35A5V1B9","RXM50A5V1B9"]
["Afmetingen","Unit","","Hoogte","mm","610","610","734"]
["","","","Breedte","mm","923","923","954"]
["","","","Diepte","mm","367","367","401"]
["Gewicht","Unit","","","kg","36","36","49"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","tpm","600","600","500"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkbereik","Koelen","Omgeving","Min.","°CDB","-10","-10","-10"]
["","","","Max.","°CDB","50","50","46 (1)"]
["","Verwarmen","Omgeving","Min.","°CWB","-21","-21","-15 (1)"]
["","","","Max.","°CWB","18","18","18"]
["Geluidsdrukniveau","Koelen","","Nom.","dBA","46","47","48"]
["","Verwarmen","","Nom.","dBA","47","49","49"]
["Koelmiddel","Type","","","","R-32","R-32","R-32"]
["","Vulling","","","kg","0.95","0.95","1.10"]
["Koudemiddel","Vulling","","","tCO2Eq","0.65","0.65","0.75"]
["Koelmiddel","GWP","","","","675","675","675"]
["Leidingaansluitingen","Leidinglengte","Max.","OU - IU","m","20","20","30"]
["","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)"]
["","Niveauverschil:","IU - OU","Max.","m","15","15","20"]
["Standaard-accessoires","RXM25A5V1B9","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Drain cap","","","","3","3","1"]
["Voeding","Fase","","","","1~","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-240"]
["Opmerkingen","","","","","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","(2) - Voor elektrische gegevens zie afzonderlijke tekening","(2) - Voor elektrische gegevens zie afzonderlijke tekening","(2) - Voor elektrische gegevens zie afzonderlijke tekening"]
["","","","","","(3) - Bevat gefluoreerde broeikasgassen","(3) - Bevat gefluoreerde broeikasgassen","(3) - Bevat gefluoreerde broeikasgassen"]
["Standaard-accessoires","RXM35A5V1B9","","","","","1"]