{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":13,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-M"]
[]
[]
[]
[]
["","","","","","RXM20M2V1B","RXM25M2V1B","RXM35M2V1B","RXM42M2V1B","RXM50M2V1B","RXM50MV1B","RXM60M2V1B","RXM71M2V1B"]
["Afmetingen","Unit","","Hoogte","mm","550","550","550","735","735","735","735","734"]
["","","","Breedte","mm","765","765","765","825","825","825","825","870"]
["","","","Diepte","mm","285","285","285","300","300","300","300","320"]
["Gewicht","Unit","","","kg","32","32","32","47","47","44","44","56"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkbereik","Koelen","Omgeving","Min.","°C DB","-10","-10","-10","-10 (1)","-10 (1)","-10","-10","-10"]
["","","","Max.","°C DB","46","46","46","46 (1)","46 (1)","46","46","46"]
["","Verwarmen","Omgeving","Min.","°CWB","-15","-15","-15","-15","-15","-15","-15","-15"]
["","","","Max.","°CWB","18","18","18","18","18","18","18","18"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","46","46","49","","","48","48"]
["","","","Nom.","dBA","","","","48","48","","","47"]
["","","","Laag","dBA","","","","","","44","44"]
["","Verwarmen","","Hoog","dBA","47","47","49","","","49","49"]
["","","","Nom.","dBA","","","","48","49","","","48"]
["","","","Laag","dBA","","","","","","45","45"]
["Koelmiddel","Type","","","","R-32","R-32","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Vulling","","","kg","0.76","0.76","0.76","1.30","1.40","1.4","1.45","1.15"]
["Koudemiddel","Vulling","","","tCO2Eq","0.5","0.5","0.5","0.88","0.95","0.9","1.0","0.78"]
["Koelmiddel","GWP","","","","675","675","675","675","675","675","675","675.0"]
["Leidingaansluitingen","Leidinglengte","Max.","OU - IU","m","30","30","30","30","30","30","30","30.0"]
["","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)"]
["","Niveauverschil:","IU - OU","Max.","m","20","20","20","20","20","20","20","20.0"]
["Standaard-accessoires","Installation manual","","","","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1"]
["","Drain plug (only heat pump models)","","","","1","1","1","","","1","1"]
["Voeding","Fase","","","","1~","1~","1~","1~","1~","1~","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50","50","50","50","50","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Standaard-accessoires","Drain plug","","","","","","","1","1","","","1"]
["Opmerkingen","","","","","","","","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","","","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["Standaard-accessoires","Drain cap","","","","","","","","","","","3"]