{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":6,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-F8"]
[]
[]
[]
[]
["","","","","","RXS71FAV1B8"]
["Ventilator","Luchtdebiet","Koelen","Superlaag","m³/min","46.0"]
["","","Verwarmen","Superlaag","m³/min","46.0"]
["","","","Superlaag","cfm","1624"]
["","","Verwarmen","Superlaag","cfm","1624"]
["Afmetingen","Unit","","Hoogte","mm","770"]
["","","","Breedte","mm","900"]
["","","","Diepte","mm","320"]
["Gewicht","Unit","","","kg","71"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","tpm","730"]
["","","Verwarmen","Superlaag","tpm","730"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor"]
["Werkbereik","Koelen","Omgeving","Min.","°CDB","-10"]
["","","","Max.","°CDB","46"]
["","Verwarmen","Omgeving","Min.","°CWB","-15"]
["","","","Max.","°CWB","18"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","52"]
["","Verwarmen","","Hoog","dBA","52"]
["Koelmiddel","Type","","","","R-410A"]
["","Vulling","","","kg","2.3"]
["Koudemiddel","Vulling","","","tCO2Eq","4.8"]
["Koelmiddel","GWP","","","","2087.5"]
["Leidingaansluitingen","Leidinglengte","Max.","OU - IU","m","30"]
["","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 10 m)"]
["","Niveauverschil:","IU - OU","Max.","m","20"]
["Standaard-accessoires","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["","Drain socket assy","","","","1"]
["Voeding","Fase","","","","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50"]
["","Spanning","","","V","220-240"]
["Opmerkingen","","","","","(1) - 220V"]
["","","","","","(2) - 230V"]
["","","","","","(3) - 240V"]