{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":73,"n_cols":11,"rows_kept":73,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L"]
[]
[]
[]
[]
["","","","","","RXS20L2V1B","RXS25L2V1B","RXS35L2V1B","RXS42L2V1B","RXS50L2V1B","RXS60L2V1B"]
["Geluidsdrukniveau","Verwarmen","","Hoog","dBA","47","47","48","48"]
["","Koelen","","Hoog","dBA","46","46","48","48"]
["Standaard-accessoires","Afvoerdop","","","","1","1","","1"]
["","Montagehandleiding","","","","1","1","1","1"]
["","Tabel koelmiddelvulling","","","","1","1","1"]
["","Meertalige labels gefluoreerde broeikasgassen","","","","1","1","Meertalige labels gefluoreerde broeikasgassen"]
["Koelmiddel","Charge","","","TCO2Eq","2.1","2.1","2.5","2.7"]
["","GWP","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["","Vulling","","","kg","1.0","1.0","1.20","1.3"]
["","Type","","","","R-410A","R-410A","R-410A","R-410A"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","tpm_","780","780","780","790"]
["","","Verwarmen","Superlaag","tpm_","740","740","740","780"]
["Werkbereik","Koelen","Omgeving","Max.","°CDB","46","46","46","46"]
["","","","Min.","°CDB","-10","-10","-10","-10"]
["","Verwarmen","Omgeving","Max.","°CWB","18","18","18","18"]
["","","","Min.","°CWB","-15","-15","-15","-15"]
["Leidingaansluitingen","Niveauverschil:","IU - OU","Max.","m","","","15"]
["","Bijkomende koelmiddelvulling","","","kg/m","","","0,020 (voor leidinglengte van meer dan 10 m)"]
["Afmetingen","Unit","","Breedte","mm","765","765","765","765"]
["","","","Diepte","mm","285","285","285","285"]
["","","","Hoogte","mm","550","550","550","550"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Gewicht","Unit","","","kg","34","34","34","39"]
["Ventilator","Luchtdebiet","Verwarmen","Superlaag","cfm","904","904","904","960"]
["","","","Superlaag","m³/min","25.6","25.6","25.6","27.2"]
["","","Koelen","Superlaag","m³/min","30.1","30.1","30.1","30.6"]
["","","","Superlaag","cfm","1,063","1,063","1,063","1,080"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Frequentie","","","Hz","50","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-240","220-240"]
["Opmerkingen","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - Bevat gefluoreerde broeikasgassen","(4) - Bevat gefluoreerde broeikasgassen","(4) - Bevat gefluoreerde broeikasgassen","(4) - Bevat gefluoreerde broeikasgassen"]
["Standaard-accessoires","Aftapplug","","","","","","1"]
["Ventilator","Luchtdebiet","Koelen","Superlaag","m³/min","","","","","48.9","45.0"]
["","","Verwarmen","Superlaag","m³/min","","","","","43.1","46.3"]
["","","","Superlaag","cfm","","","","","1727","1589"]
["","","Verwarmen","Superlaag","cfm","","","","","1522","1635"]
["Afmetingen","Unit","","Hoogte","mm","","","","","735","735"]
["","","","Breedte","mm","","","","","825","825"]
["","","","Diepte","mm","","","","","300","300"]
["Gewicht","Unit","","","kg","","","","","47","48"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","tpm_","","","","","670"]
["","","Verwarmen","Superlaag","tpm_","","","","","670"]
["Compressor","Type","","","","","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkbereik","Koelen","Omgeving","Min.","°CDB","","","","","-10","-10"]
["","","","Max.","°CDB","","","","","46","46"]
["","Verwarmen","Omgeving","Min.","°CWB","","","","","-15","-15"]
["","","","Max.","°CWB","","","","","18","18"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","","","","","48","49"]
["","","","Laag","dBA","","","","","44","46"]
["","Verwarmen","","Hoog","dBA","","","","","48","49"]
["","","","Laag","dBA","","","","","45","46"]
["Koelmiddel","Type","","","","","","","","R-410A","R-410A"]
["","Vulling","","","kg","","","","","1.7","1.5"]
["Koudemiddel","Vulling","","","tCO2Eq","","","","","3.5","3.1"]
["Koelmiddel","GWP","","","","","","","","2087.5","2087.5"]
["Leidingaansluitingen","Leidinglengte","Max.","OU - IU","m","","","","","30","30"]
["","Bijkomende koelmiddelvulling","","","kg/m","","","","","0,020 (voor leidinglengte van meer dan 10 m)","0,020 (voor leidinglengte van meer dan 10 m)"]
["","Niveauverschil:","IU - OU","Max.","m","","","","","20.0","20"]
["Standaard-accessoires","Installation manual","","","","","","","","1","1"]
["","Drain plug","","","","","","","","1","1"]
["Voeding","Fase","","","","","","","","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","","","","","50","50"]
["","Spanning","","","V","","","","","220-230-240","220-230-240"]
["Opmerkingen","","","","","","","","","","(1) - 230V"]