{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":72,"n_cols":8,"rows_kept":72,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-L3"]
[]
[]
[]
[]
["","","","","","RXS20L3V1B","RXS25L3V1B","RXS35L3V1B"]
["Geluidsdrukniveau","Verwarmen","","Hoog","dBA","","","48"]
["","Koelen","","Hoog","dBA","","","48"]
["Standaard-accessoires","Montagehandleiding","","","","","","1"]
["","Tabel koelmiddelvulling","","","","","","1"]
["","Meertalige labels gefluoreerde broeikasgassen","","","","","","1"]
["","Drainageplug (alleen warmtepompmodellen)","","","","","","1"]
["Koelmiddel","Charge","","","TCO2Eq","","","2.5"]
["","GWP","","","","","","2,087.5"]
["","Vulling","","","kg","","","1.2"]
["","Type","","","","","","R-410A"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","tpm","","","780"]
["","","Verwarmen","Superlaag","tpm","","","740"]
["Bedrijfsbereik","Koelen","Omgeving","Max.","°CDB","","","46"]
["","","","Min.","°CDB","","","-10"]
["","Verwarmen","Omgeving","Max.","°CWB","","","18"]
["","","","Min.","°CWB","","","-15"]
["Leidingaansluitingen","Hoogteverschil","IU - OU","Max.","m","","","15"]
["","Bijkomende koelmiddelvulling","","","kg/m","","","0,02 (voor leidinglengte van meer dan 10 m)"]
["Afmetingen","Unit","","Breedte","mm","","","765"]
["","","","Diepte","mm","","","285"]
["","","","Hoogte","mm","","","550"]
["Compressor","Type","","","","","","Hermetisch gesloten swingcompressor"]
["Gewicht","Unit","","","kg","","","34"]
["Ventilator","Luchtdebiet","Verwarmen","Superlaag","cfm","","","904"]
["","","","Superlaag","m³/min","","","25.6"]
["","","Koelen","Superlaag","m³/min","","","30.1"]
["","","","Superlaag","cfm","","","1,063"]
["Power supply","Phase","","","","","","1~"]
["","Frequentie","","","Hz","","","50"]
["","Spanning","","","V","","","220-240"]
["Opmerkingen","","","","","","","(1) - SL: de geluidsarme instelling van de ventilator van de luchtcirculatie"]
["Ventilator","Luchtdebiet","Koelen","Superlaag","m³/min","30.1","30.1"]
["","","Verwarmen","Superlaag","m³/min","25.6","25.6"]
["","","","Superlaag","cfm","1063","1063"]
["","","Verwarmen","Superlaag","cfm","904","904"]
["Afmetingen","Unit","","Hoogte","mm","550","550"]
["","","","Breedte","mm","765","765"]
["","","","Diepte","mm","285","285"]
["Gewicht","Unit","","","kg","34","34"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","tpm","780","780"]
["","","Verwarmen","Superlaag","tpm","740","740"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkbereik","Koelen","Omgeving","Min.","°CDB","-10","-10"]
["","","","Max.","°CDB","46","46"]
["","Verwarmen","Omgeving","Min.","°CWB","-15","-15"]
["","","","Max.","°CWB","18","18"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","46","46"]
["","Verwarmen","","Hoog","dBA","47","47"]
["Koelmiddel","Type","","","","R-410A","R-410A"]
["","Vulling","","","kg","1.0","1.0"]
["Koudemiddel","Vulling","","","tCO2Eq","2.1","2.1"]
["Koelmiddel","GWP","","","","2087.5","2087.5"]
["Leidingaansluitingen","Leidinglengte","Max.","OU - IU","m","20","20"]
["","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 10 m)","0,02 (voor leidinglengte van meer dan 10 m)"]
["","Niveauverschil:","IU - OU","Max.","m","15","15"]
["Standaard-accessoires","Installation manual","","","","1","1"]
["","Refrigerant charge label","","","","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1"]
["","Drain plug","","","","1"]
["Voeding","Fase","","","","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50","50"]
["","Spanning","","","V","220-240","220-240"]
["Opmerkingen","","","","","(1) - 220V"]
["","","","","","(2) - 230V"]
["","","","","","(3) - 240V"]
["Standaard-accessoires","Drain plug (only heat pump models)","","","","","1"]