{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":6,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXTJ-A"]
[]
[]
[]
[]
["","","","","","RXTJ30A2V1B"]
["Afmetingen","Unit","","Hoogte","mm","605"]
["","","","Breedte","mm","930"]
["","","","Diepte","mm","376"]
["Gewicht","Unit","","","kg","42"]
["Ventilatormotor","Snelheid","Koelen","Superlaag","tpm_","800"]
["","","Verwarmen","Superlaag","tpm_","400"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor"]
["Werkbereik","Koelen","Omgeving","Min.","°CDB","-10"]
["","","","Max.","°CDB","46"]
["","Verwarmen","Omgeving","Min.","°CWB","-31"]
["","","","Max.","°CWB","18"]
["Geluidsdrukniveau","Koelen","","Nom.","dBA","48"]
["","Verwarmen","","Nom.","dBA","49.0"]
["Koelmiddel","Type","","","","R-32"]
["","Vulling","","","kg","0.97"]
["Koudemiddel","Vulling","","","tCO2Eq","0.66"]
["Koelmiddel","GWP","","","","675.0"]
["Leidingaansluitingen","Leidinglengte","Max.","OU - IU","m","20"]
["","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 10 m)"]
["","Niveauverschil:","IU - OU","Max.","m","15.0"]
["Standaard-accessoires","Installation manual","","","","1"]
["","Refrigerant charge label","","","","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1"]
["Voeding","Fase","","","","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50"]
["","Spanning","","","V","220-240"]