{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":11,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXZ-N"]
[]
[]
[]
[]
["","","","","","RXZ25NV1B","RXZ25NV1B9","RXZ35NV1B9","RXZ35NV1B","RXZ50NV1B9","RXZ50NV1B"]
["Afmetingen","Unit","","Hoogte","mm","693","693","693","693","693","693"]
["","","","Breedte","mm","795","795","795","795","795","795"]
["","","","Diepte","mm","300","300","300","300","300","300"]
["Gewicht","Unit","","","kg","50","50","50","50","50","50"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkbereik","Koelen","Omgeving","Min.","°CDB","-10","-10","-10","-10","-10","-10"]
["","","","Max.","°CDB","43","43","43","43","43","43"]
["","Verwarmen","Omgeving","Min.","°CWB","-20","-20","-20","-20","-20","-20"]
["","","","Max.","°CWB","18","18","18","18","18","18"]
["Geluidsdrukniveau","Koelen","","Hoog","dBA","46","46","48","48","49","49"]
["","Verwarmen","","Hoog","dBA","46","46","48","48","50","50"]
["Koelmiddel","Type","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Vulling","","","kg","1.34","1.34","1.34","1.34","1.34","1.34"]
["Koudemiddel","Vulling","","","tCO2Eq","0.9","0.9","0.9","0.9","0.9","0.9"]
["Koelmiddel","GWP","","","","675","675","675","675","675","675"]
["Leidingaansluitingen","Leidinglengte","Max.","OU - IU","m","10","10","10","10","10","10"]
["","Niveauverschil:","IU - OU","Max.","m","8","8","8","8","8","8"]
["Standaard-accessoires","Installation manual","","","","1","1","1","1","1","1"]
["","Operation manual","","","","1","1","1","1","1","1"]
["Voeding","Fase","","","","1~","1~","1~","1~","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50","50","50","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Opmerkingen","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]