{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":8,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-B"]
[]
[]
[]
[]
["","","","","","RZAG35B5V1B","RZAG50B5V1B","RZAG60B5V1B"]
["Afmetingen","Unit","","Hoogte","mm","734","734","734"]
["","","","Breedte","mm","870","870","870"]
["","","","Diepte","mm","373","373","373"]
["Gewicht","Unit","","","kg","52","52","52"]
["Compressor","Type","","","","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor","Hermetisch gesloten swingcompressor"]
["Werkbereik","Koelen","Omgeving","Min.","°C DB","-20","-20","-20"]
["","","","Max.","°C DB","52","52","52"]
["","Verwarmen","Omgeving","Min.","°CWB","-21","-21","-21"]
["","","","Max.","°CWB","18","18","18"]
["Geluidsvermogenniveau","Koelen","","","dBA","62","63","64"]
["","Verwarmen","","","dBA","62","63","64"]
["Geluidsdrukniveau","Koelen","","Nom.","dBA","48","49","50"]
["","Verwarmen","","Nom.","dBA","48","49","50"]
["Koelmiddel","Type","","","","R-32","R-32","R-32"]
["","Vulling","","","kg","1.55","1.55","1.55"]
["","GWP","","","","675","675","675"]
["Koudemiddel","Vulling","","","tCO2Eq","1.05","1.05","1.05"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","6.35","6.35","6.35"]
["","Gas","","Buitendiameter","mm","9.52","12.7","12.7"]
["","Leidinglengte","Max.","OU - IU","m","50","50","50"]
["","Bijkomende koelmiddelvulling","","","kg/m","0,02 (voor leidinglengte van meer dan 30 m)","0,02 (voor leidinglengte van meer dan 30 m)","0,02 (voor leidinglengte van meer dan 30 m)"]
["","Niveauverschil:","IU - OU","Max.","m","30","30","30"]
["Standaard-accessoires","RZAG35B5V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","General safety precautions","General safety precautions","General safety precautions"]
["","LOT10 Energy Label","","","","LOT10 Energy Label","LOT10 Energy Label","LOT10 Energy Label"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Voeding","Fase","","","","1~","1~","1~"]
["Spanningsvoeding","Frequentie","","","Hz","50","50","50"]
["","Spanning","","","V","220-240","220-240","220-240"]
["Opmerkingen","","","","","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik","(1) - Zie afzonderlijke afbeelding voor bedrijfsbereik"]
["","","","","","(2) - Voor elektrische gegevens zie afzonderlijke tekening","(2) - Voor elektrische gegevens zie afzonderlijke tekening","(2) - Voor elektrische gegevens zie afzonderlijke tekening"]
["","","","","","(3) - Bevat gefluoreerde broeikasgassen","(3) - Bevat gefluoreerde broeikasgassen","(3) - Bevat gefluoreerde broeikasgassen"]
["Standaard-accessoires","RZAG50B5V1B","","","","","1"]
["","RZAG60B5V1B","","","","","","1"]