{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":57,"n_cols":7,"rows_kept":57,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-C"]
[]
[]
[]
[]
["","","","","","RZQ200C7Y1B","RZQ250C7Y1B"]
["Afmetingen","Unit","","Hoogte","mm","1,680"]
["","","","Breedte","mm","930"]
["","","","Diepte","mm","765"]
["Gewicht","Unit","","","kg","183.0"]
["Compressor","Type","","","","Hermetisch gesloten scrollcompressor"]
["Bedrijfsbereik","Koelen","Omgeving","Min.","°C DB","-5.0"]
["","","","Max.","°C DB","46.0"]
["","Verwarmen","Omgeving","Min.","°CWB","-15.0"]
["","","","Max.","°CWB","15.0"]
["Sound power level","Koelen","","","dBA","78.0"]
["","Verwarmen","","","dBA","78.0"]
["Koelmiddel","Type","","","","R-410A"]
["","Vulling","","","kg","8.3"]
["","GWP","","","","2,087.5"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","9.52"]
["","Gas","","Buitendiameter","mm","22.2"]
["","Leidinglengte","Max.","OU - IU","m","100"]
["","","Systeem","Zonder lading","m","30"]
["Standaard-accessoires","Montagehandleiding","","","","1"]
["","Aansluitleidingen","","","","4"]
["Power supply","Phase","","","","3N~"]
["","Frequentie","","","Hz","50"]
["","Spanning","","","V","380-415"]
["Stroom - 50Hz","Maximaal zekeringamperage (MFA)","","","A","25"]
["Opmerkingen","","","","","(1) - FDQ binnenunit heeft een afzonderlijke voeding"]
["","","","","","(2) - Voor elektrische gegevens zie afzonderlijke tekeningen"]
["Afmetingen","Unit","","Hoogte","mm","","1680"]
["","","","Breedte","mm","","930"]
["","","","Diepte","mm","","765"]
["Gewicht","Unit","","","kg","","184.0"]
["Compressor","Type","","","","","Hermetisch gesloten scrollcompressor"]
["Werkbereik","Koelen","Omgeving","Min.","°C DB","","-5.0"]
["","","","Max.","°C DB","","46.0"]
["","Verwarmen","Omgeving","Min.","°CWB","","-15.0"]
["","","","Max.","°CWB","","15.0"]
["Geluidsvermogenniveau","Koelen","","","dBA","","78.0"]
["","Verwarmen","","","dBA","","78.0"]
["Koelmiddel","Type","","","","","R-410A"]
["","Vulling","","","kg","","9.3"]
["","GWP","","","","","2087.5"]
["Koudemiddel","Vulling","","","tCO2Eq","","19.4"]
["Leidingaansluitingen","Vloeistof","","Buitendiameter","mm","","12.70"]
["","Gas","","Buitendiameter","mm","","22.2"]
["","Leidinglengte","Max.","OU - IU","m","","100"]
["","","Systeem","Zonder lading","m","","30"]
["Standaard-accessoires","Installation manual","","","","","1"]
["","Connection pipes","","","","","4"]
["Voeding","Fase","","","","","3N~"]
["Spanningsvoeding","Frequentie","","","Hz","","50"]
["","Spanning","","","V","","380-415"]
["Stroom: 50 Hz","Maximaal zekeringamperage (MFA)","","","A","","25"]