{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-AT"]
[]
[]
[]
[]
["","","","","CTXA15A2V1BT"]
["Geluidsdrukniveau","Verwarmen","Hoog","dBA","39"]
["","","Middelhoog","dBA","32"]
["","","Fluisterstille werking","dBA","21"]
["","","Laag","dBA","25"]
["","Koelen","Middelhoog","dBA","32"]
["","","Fluisterstille werking","dBA","21"]
["","","Laag","dBA","25"]
["","","Hoog","dBA","39"]
["Standaard-accessoires","Montagehandleiding","","","1"]
["","Bedieningshandleiding","","","1"]
["","Luchtfilter","","","2"]
["","Infrarood-afstandsbediening","","","1"]
["","Montageplaat afstandsbediening","","","1"]
["","Zakje schroeven","","","1"]
["","Schroefdeksel","","","1"]
["","AAA drogecelbatterij","","","2"]
["","Algemene voorzorgsmaatregelen","","","1"]
["Koelmiddel","GWP","","","675.0"]
["Regelsystemen","Bedrade afstandsbediening","","","BRC073"]
["","Infrared remote control","","","ARC466A58"]
["Piping connections","Vloeistof","Buitendiameter","mm","6.35"]
["","Gas","Buitendiameter","mm","9.50"]
["","Drainage","","","18"]
["Opgenomen vermogen","Koelen","Nom.","kW","0.020"]
["","Verwarmen","Nom.","kW","0.020"]
["Geluidsvermogenniveau","Koelen","","dBA","57"]
["Afmetingen","Unit","Breedte","mm","798"]
["","","Diepte","mm","189"]
["","","Hoogte","mm","295"]
["Behuizing","Colour","","","Zwart hout"]
["Gewicht","Unit","","kg","12"]
["Power supply","Fase","","","1~"]
["","Frequentie","","Hz","50"]
["","Naam","","","V1"]
["","Spanning","","V","220-240"]