{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":11,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C"]
[]
[]
[]
[]
["","","","","FHQ35CAVEB","FHQ50CAVEB","FHQ60CAVEB","FHQ71CAVEB","FHQ100CAVEB","FHQ125CAVEB","FHQ140CAVEB"]
["Geluidsdrukniveau","Verwarmen","Hoog","dBA","36","37","37","38","42","44","46"]
["","","Nom.","dBA","34","35","35","36","38","41","42"]
["","","Laag","dBA","31","32","33","34","34","37","38"]
["","Koelen","Laag","dBA","31","32","33","34","34","37","38"]
["","","Hoog","dBA","36","37","37","38","42","44","46"]
["","","Nom.","dBA","34","35","35","36","38","41","42"]
["Standaard-accessoires","Montagehandleiding","","","Montagehandleiding","Montagehandleiding","Montagehandleiding","Montagehandleiding","Montagehandleiding","Montagehandleiding","Montagehandleiding"]
["","Bedieningshandleiding","","","Bedieningshandleiding","Bedieningshandleiding","Bedieningshandleiding","Bedieningshandleiding","Bedieningshandleiding","Bedieningshandleiding","Bedieningshandleiding"]
["","Verklaring van conformiteit","","","Verklaring van conformiteit","Verklaring van conformiteit","Verklaring van conformiteit","Verklaring van conformiteit","Verklaring van conformiteit","Verklaring van conformiteit","Verklaring van conformiteit"]
["","Afvoerslang","","","Afvoerslang","Afvoerslang","Afvoerslang","Afvoerslang","Afvoerslang","Afvoerslang","Afvoerslang"]
["","Klemmetaal","","","Klemmetaal","Klemmetaal","Klemmetaal","Klemmetaal","Klemmetaal","Klemmetaal","Klemmetaal"]
["","Sluitring voor ophangbeugel","","","Sluitring voor ophangbeugel","Sluitring voor ophangbeugel","Sluitring voor ophangbeugel","Sluitring voor ophangbeugel","Sluitring voor ophangbeugel","Sluitring voor ophangbeugel","Sluitring voor ophangbeugel"]
["","Klemmen","","","Klemmen","Klemmen","Klemmen","Klemmen","Klemmen","Klemmen","Klemmen"]
["","Montagepatroon","","","Montagepatroon","Montagepatroon","Montagepatroon","Montagepatroon","Montagepatroon","Montagepatroon","Montagepatroon"]
["","Isolatiemateriaal koppelverbindingen","","","Isolatiemateriaal koppelverbindingen","Isolatiemateriaal koppelverbindingen","Isolatiemateriaal koppelverbindingen","Isolatiemateriaal koppelverbindingen","Isolatiemateriaal koppelverbindingen","Isolatiemateriaal koppelverbindingen","Isolatiemateriaal koppelverbindingen"]
["","Afdichtingsmateriaal","","","Afdichtingsmateriaal","Afdichtingsmateriaal","Afdichtingsmateriaal","Afdichtingsmateriaal","Afdichtingsmateriaal","Afdichtingsmateriaal","Afdichtingsmateriaal"]
["","Mof van kunsthars","","","Mof van kunsthars","Mof van kunsthars","Mof van kunsthars","Mof van kunsthars","Mof van kunsthars","Mof van kunsthars","Mof van kunsthars"]
["","Bedradingsklem","","","Bedradingsklem","Bedradingsklem","Bedradingsklem","Bedradingsklem","Bedradingsklem","Bedradingsklem","Bedradingsklem"]
["","Schroef voor vastklemmen van draden","","","Schroef voor vastklemmen van draden","Schroef voor vastklemmen van draden","Schroef voor vastklemmen van draden","Schroef voor vastklemmen van draden","Schroef voor vastklemmen van draden","Schroef voor vastklemmen van draden","Schroef voor vastklemmen van draden"]
["Besturingssystemen","Wired remote control","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53","BRC7G53"]
["Leidingaansluitingen","Vloeistof","Buitendiameter","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Gas","Buitendiameter","mm","9.5","12.7","12.7","15.9","15.9","15.9","15.9"]
["","Afvoer","","","VP20","VP20","VP20","VP20","VP20","VP20","VP20"]
["Geluidsvermogenniveau","Koelen","","dBA","53","54","54","55","60","62","64"]
["","Verwarmen","","dBA","53","54","54","55","60","62","64"]
["Afmetingen","Unit","Breedte","mm","960","960","1,270","1,270","1,590","1,590","1,590"]
["","","Diepte","mm","690","690","690","690","690","690","690"]
["","","Hoogte","mm","235","235","235","235","235","235","235"]
["Casing","Material","","","Kunsthars, metaalplaat","Kunsthars, metaalplaat","Kunsthars, metaalplaat","Kunsthars, metaalplaat","Kunsthars, metaalplaat","Kunsthars, metaalplaat","Kunsthars, metaalplaat"]
["","Colour","","","Zuiver wit","Zuiver wit","Zuiver wit","Zuiver wit","Zuiver wit","Zuiver wit","Zuiver wit"]
["Gewicht","Unit","","kg","24","25","31","32","38","38","38"]
["Power supply","Phase","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frequentie","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Naam","","","VE","VE","VE","VE","VE","VE","VE"]
["","Spanning","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]